**ASSIGNMENT-4**

**Q**

Write code and connections in wokwi for ultrasonic.When ever distance Isless than 100 cm end“alert”to ibm cloud and display in device recent events.

**SOLUTION**

#include <WiFi.h>//library for wifi

#include <PubSubClient.h>//library for MQtt

#define EchoPIN 4     // what pin we're connected to

#define TrigPIN 2

#define LED 5

//DHT dht (DHTPIN, DHTTYPE);// creating the instance by passing pin and typr of dht connected

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "swz5ou"//IBM ORGANITION ID

#define DEVICE\_TYPE "abcd"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "12"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "12345678"     //Token

String data3;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name

char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/command/fmt/String";// cmd  REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING

char authMethod[] = "use-token-auth";// authentication method

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id

float dist,dur;

String data;

//-----------------------------------------

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

void setup()// configureing the ESP32

{

**Serial**.begin(115200);

  pinMode(TrigPIN, OUTPUT);

  digitalWrite(TrigPIN, LOW);

  pinMode(EchoPIN, INPUT);

  pinMode(LED,OUTPUT);

  delay(10);

**Serial**.println();

  wificonnect();

  mqttconnect();

}

void loop()// Recursive Function

{

  digitalWrite(TrigPIN, HIGH);

  delayMicroseconds(10);

  digitalWrite(TrigPIN, LOW);

  dur = pulseIn(EchoPIN,HIGH);

  dist= dur \*0.034 / 2;

if(dist<100)

  {

    data="alert";

    digitalWrite(LED,HIGH);

  }

  else{

    data="safe";

    digitalWrite(LED,LOW);

  }

  PublishData(dist);

  delay(1000);

  if (!client.loop()) {

    mqttconnect();

  }

}

/\*.....................................retrieving to Cloud...............................\*/

void PublishData(float dist) {

  mqttconnect();//function call for connecting to ibm

  /\*

     creating the String in in form JSon to update the data to ibm cloud

  \*/

  String payload = "{\"distance\":";

  payload += dist;

  payload += "," "\"msg\":\"";

  payload += data;

  payload += "\"}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

  if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");// if it sucessfully upload data on the cloud then it will print publish ok in Serial monitor or else it will print publish failed

  } else {

**Serial**.println("Publish failed");

  }

}

void mqttconnect() {

  if (!client.connected()) {

**Serial**.print("Reconnecting client to ");

**Serial**.println(server);

    while (!!!client.connect(clientId, authMethod, token)) {

**Serial**.print(".");

      delay(500);

    }

     initManagedDevice();

**Serial**.println();

  }

}

void wificonnect() //function defination for wificonnect

{

**Serial**.println();

**Serial**.print("Connecting to ");

  WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

  while (WiFi.status() != WL\_CONNECTED) {

    delay(500);

**Serial**.print(".");

  }

**Serial**.println("");

**Serial**.println("WiFi connected");

**Serial**.println("IP address: ");

**Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

  if (client.subscribe(subscribetopic)) {

**Serial**.println((subscribetopic));

**Serial**.println("subscribe to cmd OK");

  } else {

**Serial**.println("subscribe to cmd FAILED");


  }

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

}



**Wokwi Link:** <https://wokwi.com/projects/348296026455540307>

**IBM Cloud**

**Device Recent Events**

